#Verisafe Network Module Release Notes

v1.0.2:
	Production Release

v1.0.3:		
	-Corrected issue where selecting https mode and using a custom certificate could show "Error Requesting Settings" message.
	
v2.0.1:
	-Added the ability to remotely activate an AVT test from the web interface, EtherNet/IP and Modbus TCP
	-Added current temperature reading from the AVT, available from the web interface, EtherNet/IP and Modbus TCP
	-Updated EtherNet/IP and Modbus TCP data models to incorporate remote test activation and current temperature parameters
	-Improved voltage accuracy reporting below 50V with new power system configuration selection options
	-Changed the default web server mode to HTTPS
	-Addressed several security vulnerabilities identified by WebInspect
	-Added open-source license acknowledgements to the web interface
	-Updated data log formatting
	-Updated info on support page
	
	Note: Network Module Firmware version 2.0.1 must be used with AVT Isolation Module Voltage Presence firmware 2.0.0 or later.
	      For use with EtherNet/IP and Studio 5000, use Rockwell VeriSafe AOP version 2.01.03
